{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"images":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":7,"n_cols":6,"rows_kept":7,"merged":[[0,0,0,5],[2,2,5,2],[2,3,5,3],[2,4,5,4],[2,5,3,5],[6,0,6,5]],"flags":["formulas_cached_only"]}
["实木套装门（含安装）"]
["品类","详情","单樘门不含税控制单价(元/樘)","子母门不含税控制单价(元/樘)","对开门单价(元/樘)","备注"]
["木门","门扇/门套/门边线：\n规格：门扇厚度45mm，门套厚度35mm，门边线宽度70mm 厚度12到14mm；(门扇和门套高宽按现场测量尺寸生产为准）具有极强的抗震性能和减震性能。结构牢固，性能稳定，抗变形、防潮、耐磨度强。                                                         1、基材：实木内架，实木多层板，该产品通过国家环境标志产品检验检测，符合“十环产品认证”标准，经过耐酸碱、防虫、防腐特殊处理，抗弯力强，不易变形，有害物质限量低于GB18584-2001要求。                                                                                           2、面材：三聚氢胺纸饰面，饰面纸符合LY/T1831-2009人造板饰面专用装饰纸相关要求；                                                 \n3、实木填芯：多层实木","1350元/樘","2000元/樘","2400元/樘","单樘门尺寸900X2100   "]
[null,"消音条：\n规格：宽度10mm，厚度5mm；\n材质：弹性体；"]
[null,"合页：每套门3付合页\n规格：4mm*3mm*3mm;\n材质：304不锈钢；\n表面处理：拉丝；",{"$nulls":3},"单门83樘"]
[null,"门吸：\n规格：高88mm，直径42mm；\n材质：304不锈钢；\n表面处理：拉丝",{"$nulls":3},"对开门2樘"]
["说明：1、报价为单价包干：包含成品材料费、运输费、上下车费、辅材费、安装费等一切费用；\n2、质量保证期不得低于2年；\n3、最终结算工程量，以实际收方单据为准；\n4、服务期内供货价不得高于投标时最终报价；\n5、下单起2023年3月25日前安装完成。"]